{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Calculations","Table"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Calculations","index":0,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":false,"merged":[[0,0,0,2],[1,0,1,2]]}
["КОНВЕРТОР / CONVERTER\ntСО2 еквивалент ↔ Количество ФПГ               \n tCO2 equivalent ↔ F-gas quantity\n"]
[]
[]
[]
[]
["вид фреон\n refrigerant type","количество/quantity\nkg","tCO2 еквивалент  \ntCO2 equivalent"]

{"sheet":"Table","index":1,"n_rows":24,"n_cols":2,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Refrigerant","GWP"]
["R134a",1430]
["R32",675]
["R404A",3921.6000000000004]
["R407A",2107]
["R407C",1773.85]
["R407D",1627]
["R407F",1824.5]
["R410A",2087.5]
["R413A",2053.2199999999998]
["R417A",2346]
["R422A",3143.0859999999998]
["R422D",2729.0859999999998]
["R424A",2440]
["R426A",1508]
["R427A",2138.25]
["R428A",3607]
["R434A",3246]
["R437A",1805]
["R438A",2265]
["R442A",1888]
["R507",3985]
["R508A",13214]
["R508B",13396]